

Begin Communication with PICCActivate
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
>>  50 00 02 22 10 26 46
The Bytes in Detail:
50    = Start of telegram
00 02 = 2 Bytes of payload between command code and checksum
22    = Command code
10    = 10 ms antenna pause for chip reset
26    = Request IDLE
46    = Checksum




Now Communicate using direct PICCTRANSFER
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯

FAST_READ (Chapter 10.3 page 23)

>>  50 00 03 2E 3A 00 06 41
The Bytes in Detail:
50    = Start of telegram
00 03 = 3 Bytes of payload between command code and checksum
2E    = PICCTRANSFER
3A    = FAST_READ
00    = Start Page Number
06    = End Page Number
41    = Checksum


